Test of the **SAMD** boards

Catena\_hello.ino 🡪 board (SAMD) 🡪 4410

Catena\_hello.ino 🡪 board (SAMD) 🡪4420

Catena\_hello.ino 🡪 board (SAMD) 🡪4450

Catena\_hello.ino 🡪 board (SAMD) 🡪4460

Catena\_hello.ino 🡪 board (SAMD) 🡪4470

Test the user-command example & the fsm example on the 4470

Catena\_usercommand.ino 🡪 board (SAMD) 🡪4470

Catena\_fsm.ino 🡪 board (SAMD) 🡪 4470

Test each of the regions on the 4450.

Catena\_hello\_lora.ino 🡪 board (4450) 🡪 Region ( us915 , eu868 , au915 , as923 , as923jp , in866)

Test each of the STM32L0 boards

Catena\_hello.ino 🡪 board (STM32) 🡪4551

Catena\_hello\_lora.ino 🡪 board (STM32) 🡪4551

Catena\_hello.ino 🡪 board (STM32) 🡪4610

Catena\_hello\_lora.ino 🡪 board (STM32) 🡪4610

Catena\_hello.ino 🡪 board (STM32) 🡪4611

Catena\_hello\_lora.ino 🡪 board (STM32) 🡪4611

Catena\_hello.ino 🡪 board (STM32) 🡪4612

Catena\_hello\_lora.ino 🡪 board (STM32) 🡪4612

Catena\_hello.ino 🡪 board (STM32) 🡪4617

Catena\_hello\_lora.ino 🡪 board (STM32) 🡪4617

Catena\_hello.ino 🡪 board (STM32) 🡪4618

Catena\_hello\_lora.ino 🡪 board (STM32) 🡪4618

Catena\_hello.ino 🡪 board (STM32) 🡪46 30

Catena\_hello\_lora.ino 🡪 board (STM32) 🡪4630

Catena\_hello.ino 🡪 board (STM32) 🡪4801

Catena\_hello\_lora.ino 🡪 board (STM32) 🡪4801

Test the user-command and fsm examples on the 4610

Catena\_usercommand.ino 🡪 board (STM32) 🡪4610

Catena\_fsm.iio 🡪 board (STM32) 🡪4610

Test each of the regions for 4610 (using it as an example). us915 already tested

Catena\_hello\_lora.ino 🡪 board (STM32)🡪 4610 🡪 Region (eu868)

Catena\_hello\_lora.ino 🡪 board (STM32)🡪 4610 🡪 Region (au915)

Catena\_hello\_lora.ino 🡪 board (STM32)🡪 4610 🡪 Region (as923)

Catena\_hello\_lora.ino 🡪 board (STM32)🡪 4610 🡪 Region (as923jp)

Catena\_hello\_lora.ino 🡪 board (STM32)🡪 4610 🡪 Region (in866)